BAE CHAPTER 1 LESSON SUMMARY SOUND AND HEARING

1/12/18 WEEK ONE LESSON

ROOM MEZZAINE ROOM

Day 1 1/9/18

INSTRUCTOR: MARK AND DERRICK

CLIENT : ISABELLA

OBSERVATION LESSON MIXING PROJECT NYC 134 SESSION

Ass Amplifier signal in recording bass keep one track.

Pick Colors for instrument tracks always use colors easier for catergorizing.

3.industry Standard is Pro Tools 10 But Pro Tools 12 is universal.

4.Sonic advantage is better mix on console . “ SSL 4000 GPLUS CONSOLE”

5. Mixing is Organization.

Round Robin saves to six hard drives keep track and artists stuff organized.

Signal Path= flow of signal path from mic to protools / mic = slave=compressor=cue

When using record in melodine save as in melodine and bounce to track.

Drums route to drum Bus, vocals route to vocal bus, etc.

Evertything below 70htz for sudio monitors.

Bass elements usually compress aggressively are Rock and Hip Hop.

ROOM ERA MASTERING ROOM

Day 1/10/18

INSTRUCTOR: Mark

CLIENT: ISABELLA

OBSERVATION Mastering Project NYC 134 SESSION

Instructor: Mark

LESSON NOTES:

Networking is more essiential to mastering business.

Recall sheets in mastering are used to remember the knobs in mastering session.

Tubetech is multihand compressor settings low meduim high .

TC Elctronics for low end drop out below 29 htz.

L2 Limiter 0.0DBFS (max)

ISRC ISRC.org International copyrights for codec on mastered songs.

Anacologic Chamber for recording.

3 Stages of audio engineer Teacking, Mixing, Mastering in Bae

Compressor is security to be leveled at 3 to 1

Threshold at Compressor attack release 5 higher

Virtual Instruments are already compressed.

Saturation plug in gives a distortion

Phases of MAstering Saturation plug in - distortion- tube

Distortion Tube = pushes harmony

Reverb, delay, Saturation are bad in Mastering

Spectrual Cleaning is last step in MAstering.

SeQuoia , Sade are Matering platforms

No Mastering in ProTools

Vocal Fade in and Out on all vocals.

U87 , akg c12, best mikes for hip hop.

Volume cant be measured its an experience

Avalon 747 don’t touch

Bits are to low bad recording to close to ceiling, between two extremeties

Tracking Compressor for voice , mic placement,

SPL Sound Pressue Level

Anacologic Chamber for recording